# Static Call Graph for image ..\..\Output\atk_hmi.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Wed May 29 16:09:08 2024

### Maximum Stack Usage = 600 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ hmi_update_ui_50ms ⇒ hmi_curve_example_timer_update_50ms ⇒ real_time_curve ⇒ api_caddt ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- hmi_spinner_example_hex_cmd ⇒ api_get
- hmi_slider_example_hex_cmd ⇒ api_get
- hmi_select_text_example_hex_cmd ⇒ api_get
- hmi_btn_example_hex_cmd ⇒ api_get

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - ADC3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - BusFault_Handler from stm32f1xx_it.o(i.BusFault_Handler) referenced from startup_stm32f103xe.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DebugMon_Handler from stm32f1xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f103xe.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - FLASH_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - FSMC_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - HardFault_Handler from stm32f1xx_it.o(i.HardFault_Handler) referenced from startup_stm32f103xe.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - MemManage_Handler from stm32f1xx_it.o(i.MemManage_Handler) referenced from startup_stm32f103xe.o(RESET)
  - NMI_Handler from stm32f1xx_it.o(i.NMI_Handler) referenced from startup_stm32f103xe.o(RESET)
  - PVD_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - PendSV_Handler from stm32f1xx_it.o(i.PendSV_Handler) referenced from startup_stm32f103xe.o(RESET)
  - RCC_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - RTC_IRQHandler from rtc.o(i.RTC_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - Reset_Handler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - SDIO_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - SPI1_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - SPI2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - SPI3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - SVC_Handler from stm32f1xx_it.o(i.SVC_Handler) referenced from startup_stm32f103xe.o(RESET)
  - SysTick_Handler from stm32f1xx_it.o(i.SysTick_Handler) referenced from startup_stm32f103xe.o(RESET)
  - SystemInit from system_stm32f1xx.o(i.SystemInit) referenced from startup_stm32f103xe.o(.text)
  - TAMPER_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM4_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM5_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM6_IRQHandler from main.o(i.TIM6_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - TIM7_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - UART4_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - UART5_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - UART_DMAAbortOnError from stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError) referenced from stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler)
  - USART1_IRQHandler from usart.o(i.USART1_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - USART2_IRQHandler from usart2.o(i.USART2_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - USART3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - UsageFault_Handler from stm32f1xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f103xe.o(RESET)
  - WWDG_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f103xe.o(.text)
  - _get_lc_ctype from lc_ctype_c.o(locale$$code) referenced from rt_ctype_table.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - _sbackspace from _sgetc.o(.text) referenced from __0sscanf.o(.text)
  - _scanf_char_input from scanf_char.o(.text) referenced from scanf_char.o(.text)
  - _sgetc from _sgetc.o(.text) referenced from __0sscanf.o(.text)
  - _snputc from _snputc.o(.text) referenced from noretval__2snprintf.o(.text)
  - _sputc from _sputc.o(.text) referenced from noretval__2sprintf.o(.text)
  - fputc from usart.o(i.fputc) referenced from _printf_char_file.o(.text)
  - isspace from isspace.o(.text) referenced from scanf_char.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __decompress (Thumb, 90 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __decompress1 (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_dec

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_s (Thumb, 0 bytes, Stack size unknown bytes, _printf_s.o(.ARM.Collect$$_printf_percent$$00000014))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = _printf_s ⇒ _printf_string ⇒ _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_string

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_common (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))
  [Calls]

  - >> __rt_locale

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_2 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000012))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init_lc_ctype_2 ⇒ _get_lc_ctype
  [Calls]
  - >> _get_lc_ctype

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_fini_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000011))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000012))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 600 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ hmi_update_ui_50ms ⇒ hmi_curve_example_timer_update_50ms ⇒ real_time_curve ⇒ api_caddt ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f103xe.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __use_no_semihosting (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi_2.o(.text), UNUSED)

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, noretval__2printf.o(.text))
  [Stack]

  - Max Depth = 128 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> hmi_test_init
  - >> hmi_spinner_example_hex_cmd
  - >> hmi_slider_example_hex_cmd
  - >> hmi_progerss_bar_example_timer_update_50ms
  - >> hmi_btn_example_hex_cmd

  __2sprintf (Thumb, 34 bytes, Stack size 32 bytes, noretval__2sprintf.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _sputc
  - >> _printf_char_common
  [Called By]
  - >> hmi_qr_example_hex_cmd
  - >> hmi_pointer_example_timer_update_50ms
  - >> hmi_btn_example_timer_update_50ms
  - >> hmi_btn_example_hex_cmd

  __2snprintf (Thumb, 48 bytes, Stack size 32 bytes, noretval__2snprintf.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = __2snprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _sputc
  - >> _printf_char_common
  [Called By]
  - >> api_rtcs
  - >> api_get
  - >> api_cclear
  - >> api_caddt

  __printf (Thumb, 104 bytes, Stack size 24 bytes, __printf.o(.text))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  [Called By]
  - >> _printf_char_common

  _printf_str (Thumb, 82 bytes, Stack size 16 bytes, _printf_str.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_str
  [Called By]
  - >> _printf_cs_common

  _printf_int_dec (Thumb, 104 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_d

  __0sscanf (Thumb, 52 bytes, Stack size 72 bytes, __0sscanf.o(.text))
  [Stack]

  - Max Depth = 224
  - Call Chain = __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_string
  [Calls]
  - >> __vfscanf_char
  [Called By]
  - >> _cmd_return_parse
  - >> hmi_str_cmd_parse

  _scanf_int (Thumb, 332 bytes, Stack size 56 bytes, _scanf_int.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _scanf_int
  [Calls]
  - >> _chval
  [Called By]
  - >> __vfscanf

  _scanf_string (Thumb, 224 bytes, Stack size 56 bytes, _scanf_str.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _scanf_string
  [Called By]
  - >> __vfscanf

  strchr (Thumb, 20 bytes, Stack size 0 bytes, strchr.o(.text))
  [Called By]

  - >> _buf_save_res_buf

  strstr (Thumb, 36 bytes, Stack size 12 bytes, strstr.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strstr
  [Called By]
  - >> _cmd_return_parse
  - >> real_time_curve
  - >> hmi_btn_example_str_cmd
  - >> hmi_str_cmd_parse

  strlen (Thumb, 62 bytes, Stack size 8 bytes, strlen.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strlen
  [Called By]
  - >> _buf_save_res_buf
  - >> hmi_cmd_send

  __aeabi_memmove (Thumb, 0 bytes, Stack size 0 bytes, rt_memmove_v6.o(.text))
  [Called By]

  - >> _buf_save_res_buf

  __rt_memmove (Thumb, 132 bytes, Stack size 0 bytes, rt_memmove_v6.o(.text), UNUSED)
  [Calls]

  - >> __memmove_aligned
  - >> __aeabi_memcpy

  __memmove_lastfew (Thumb, 0 bytes, Stack size unknown bytes, rt_memmove_v6.o(.text), UNUSED)

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_memclr4
  [Called By]
  - >> led0_pwm_init
  - >> hmi_qr_example_hex_cmd

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 78 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  _memset_w (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  _printf_int_common (Thumb, 178 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_int_common
  [Called By]
  - >> _printf_int_dec

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> _printf_char_file
  - >> __2snprintf
  - >> __2sprintf

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, _sputc.o(.text))
  [Called By]

  - >> __2snprintf
  - >> __2sprintf
  [Address Reference Count : 1]
  - noretval__2sprintf.o(.text)

  _snputc (Thumb, 16 bytes, Stack size 0 bytes, _snputc.o(.text))
  [Address Reference Count : 1]

  - noretval__2snprintf.o(.text)

  _printf_cs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_str
  [Called By]
  - >> _printf_string
  - >> _printf_char

  _printf_char (Thumb, 16 bytes, Stack size 0 bytes, _printf_char.o(.text), UNUSED)
  [Calls]

  - >> _printf_cs_common

  _printf_string (Thumb, 8 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _printf_string ⇒ _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_s

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ferror
  - >> _printf_char_common
  [Called By]
  - >> __2printf

  _chval (Thumb, 28 bytes, Stack size 0 bytes, _chval.o(.text))
  [Called By]

  - >> _scanf_int

  __vfscanf_char (Thumb, 24 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = __vfscanf_char ⇒ __vfscanf ⇒ _scanf_string
  [Calls]
  - >> __vfscanf
  [Called By]
  - >> __0sscanf

  _sgetc (Thumb, 30 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - __0sscanf.o(.text)

  _sbackspace (Thumb, 34 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - __0sscanf.o(.text)

  __aeabi_memcpy (Thumb, 0 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text), UNUSED)
  [Called By]

  - >> __rt_memmove

  __rt_memcpy (Thumb, 138 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4

  _memcpy_lastbytes (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_v6.o(.text), UNUSED)

  __aeabi_memmove4 (Thumb, 0 bytes, Stack size 8 bytes, rt_memmove_w.o(.text), UNUSED)

  __aeabi_memmove8 (Thumb, 0 bytes, Stack size 8 bytes, rt_memmove_w.o(.text), UNUSED)

  __rt_memmove_w (Thumb, 122 bytes, Stack size 8 bytes, rt_memmove_w.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4

  __memmove_aligned (Thumb, 0 bytes, Stack size unknown bytes, rt_memmove_w.o(.text), UNUSED)
  [Called By]

  - >> __rt_memmove

  __memmove_lastfew_aligned (Thumb, 0 bytes, Stack size unknown bytes, rt_memmove_w.o(.text), UNUSED)

  isspace (Thumb, 18 bytes, Stack size 8 bytes, isspace.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = isspace ⇒ __rt_ctype_table
  [Calls]
  - >> __rt_ctype_table
  [Address Reference Count : 1]
  - scanf_char.o(.text)

  __vfscanf (Thumb, 880 bytes, Stack size 96 bytes, _scanf.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = __vfscanf ⇒ _scanf_string
  [Calls]
  - >> _scanf_string
  - >> _scanf_int
  [Called By]
  - >> __vfscanf_char

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)
  [Called By]

  - >> __rt_memmove_w
  - >> __rt_memcpy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  __rt_memcpy_w (Thumb, 100 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  _memcpy_lastbytes_aligned (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_w.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  __rt_ctype_table (Thumb, 16 bytes, Stack size 8 bytes, rt_ctype_table.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __rt_ctype_table
  [Calls]
  - >> __rt_locale
  [Called By]
  - >> isspace

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __rt_locale (Thumb, 8 bytes, Stack size 0 bytes, rt_locale_intlibspace.o(.text))
  [Called By]

  - >> __rt_lib_init_lc_common
  - >> __rt_ctype_table

  strcmp (Thumb, 128 bytes, Stack size 0 bytes, strcmpv7m.o(.text))
  [Called By]

  - >> _get_lc_ctype

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  HAL_DMA_Abort_IT (Thumb, 414 bytes, Stack size 16 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA_Abort_IT
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_Delay (Thumb, 36 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RTC_MspInit

  HAL_GPIO_Init (Thumb, 792 bytes, Stack size 36 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_MspInit
  - >> usart2_init
  - >> led_init
  - >> led0_pwm_init
  - >> HAL_TIM_PWM_MspInit

  HAL_GPIO_TogglePin (Thumb, 14 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_TogglePin))
  [Called By]

  - >> main

  HAL_GPIO_WritePin (Thumb, 12 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> led_init

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_Delay
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> hmi_cmd_wait_parse
  - >> hmi_rx_parse_task
  - >> HAL_RTC_WaitForSynchro
  - >> RTC_ExitInitMode
  - >> RTC_EnterInitMode

  HAL_IncTick (Thumb, 16 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_MspInit
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 64 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_MspInit))
  [Called By]

  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_UART_MspInit
  - >> usart2_init
  - >> timer6_init
  - >> rtc_init

  HAL_NVIC_SetPriority (Thumb, 124 bytes, Stack size 40 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  - >> __NVIC_GetPriorityGrouping
  [Called By]
  - >> HAL_InitTick
  - >> HAL_UART_MspInit
  - >> usart2_init
  - >> timer6_init
  - >> rtc_init

  HAL_NVIC_SetPriorityGrouping (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init

  HAL_PWR_EnableBkUpAccess (Thumb, 8 bytes, Stack size 0 bytes, stm32f1xx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess))
  [Called By]

  - >> rtc_init
  - >> rtc_write_bkr
  - >> rtc_set_time

  HAL_RCCEx_GetPeriphCLKFreq (Thumb, 276 bytes, Stack size 48 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_RCCEx_GetPeriphCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_RCC_GetPCLK2Freq
  [Called By]
  - >> HAL_RTC_Init

  HAL_RCCEx_PeriphCLKConfig (Thumb, 290 bytes, Stack size 24 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RTC_MspInit

  HAL_RCC_ClockConfig (Thumb, 376 bytes, Stack size 16 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_InitTick
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_GetTick
  [Called By]
  - >> sys_stm32_clock_init

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq

  HAL_RCC_GetPCLK1Freq (Thumb, 22 bytes, Stack size 4 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_RCC_GetPCLK1Freq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 22 bytes, Stack size 4 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_RCC_GetPCLK2Freq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig
  - >> HAL_RCCEx_GetPeriphCLKFreq

  HAL_RCC_GetSysClockFreq (Thumb, 116 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_GetPeriphCLKFreq

  HAL_RCC_OscConfig (Thumb, 1114 bytes, Stack size 24 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RCC_OscConfig ⇒ RCC_Delay
  [Calls]
  - >> RCC_Delay
  - >> HAL_GetTick
  [Called By]
  - >> sys_stm32_clock_init
  - >> HAL_RTC_MspInit

  HAL_RTCEx_BKUPRead (Thumb, 20 bytes, Stack size 8 bytes, stm32f1xx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPRead))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_RTCEx_BKUPRead
  [Called By]
  - >> rtc_read_bkr

  HAL_RTCEx_BKUPWrite (Thumb, 18 bytes, Stack size 8 bytes, stm32f1xx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPWrite))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_RTCEx_BKUPWrite
  [Called By]
  - >> rtc_write_bkr

  HAL_RTC_Init (Thumb, 202 bytes, Stack size 16 bytes, stm32f1xx_hal_rtc.o(i.HAL_RTC_Init))
  [Stack]

  - Max Depth = 128
  - Call Chain = HAL_RTC_Init ⇒ HAL_RTC_MspInit ⇒ HAL_RCC_OscConfig ⇒ RCC_Delay
  [Calls]
  - >> HAL_RCCEx_GetPeriphCLKFreq
  - >> HAL_RTC_MspInit
  - >> HAL_RTC_WaitForSynchro
  - >> RTC_ExitInitMode
  - >> RTC_EnterInitMode
  [Called By]
  - >> rtc_init

  HAL_RTC_MspInit (Thumb, 144 bytes, Stack size 80 bytes, rtc.o(i.HAL_RTC_MspInit))
  [Stack]

  - Max Depth = 112
  - Call Chain = HAL_RTC_MspInit ⇒ HAL_RCC_OscConfig ⇒ RCC_Delay
  [Calls]
  - >> HAL_Delay
  - >> HAL_RCC_OscConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> rtc_write_bkr
  [Called By]
  - >> HAL_RTC_Init

  HAL_RTC_WaitForSynchro (Thumb, 64 bytes, Stack size 16 bytes, stm32f1xx_hal_rtc.o(i.HAL_RTC_WaitForSynchro))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_RTC_WaitForSynchro
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RTC_Init

  HAL_SYSTICK_Config (Thumb, 52 bytes, Stack size 16 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_SYSTICK_Config ⇒ __NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick

  HAL_TIM_Base_Init (Thumb, 52 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> timer6_init

  HAL_TIM_Base_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_MspInit))
  [Called By]

  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start_IT (Thumb, 42 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Start_IT))
  [Called By]

  - >> timer6_init

  HAL_TIM_PWM_ConfigChannel (Thumb, 264 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_PWM_ConfigChannel ⇒ TIM_OC4_SetConfig
  [Calls]
  - >> TIM_OC4_SetConfig
  - >> TIM_OC3_SetConfig
  - >> TIM_OC1_SetConfig
  - >> TIM_OC2_SetConfig
  [Called By]
  - >> led0_pwm_init

  HAL_TIM_PWM_Init (Thumb, 52 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_Init))
  [Stack]

  - Max Depth = 76
  - Call Chain = HAL_TIM_PWM_Init ⇒ HAL_TIM_PWM_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_TIM_PWM_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> led0_pwm_init

  HAL_TIM_PWM_MspInit (Thumb, 98 bytes, Stack size 32 bytes, led0_pwm.o(i.HAL_TIM_PWM_MspInit))
  [Stack]

  - Max Depth = 68
  - Call Chain = HAL_TIM_PWM_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_TIM_PWM_Init

  HAL_TIM_PWM_Start (Thumb, 80 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_Start))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_PWM_Start ⇒ TIM_CCxChannelCmd
  [Calls]
  - >> TIM_CCxChannelCmd
  [Called By]
  - >> led0_pwm_init

  HAL_UART_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_ErrorCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_DMAAbortOnError

  HAL_UART_GetState (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_GetState))
  [Called By]

  - >> USART1_IRQHandler

  HAL_UART_IRQHandler (Thumb, 326 bytes, Stack size 32 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_UART_IRQHandler ⇒ HAL_DMA_Abort_IT
  [Calls]
  - >> HAL_DMA_Abort_IT
  - >> HAL_UART_ErrorCallback
  - >> UART_Transmit_IT
  - >> UART_Receive_IT
  - >> UART_EndTransmit_IT
  - >> UART_EndRxTransfer
  [Called By]
  - >> USART1_IRQHandler
  - >> USART2_IRQHandler

  HAL_UART_Init (Thumb, 114 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> usart_init
  - >> usart2_init

  HAL_UART_MspInit (Thumb, 168 bytes, Stack size 32 bytes, usart.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_UART_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Receive_IT (Thumb, 112 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Receive_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_UART_Receive_IT
  [Called By]
  - >> USART1_IRQHandler
  - >> usart_init

  HAL_UART_RxCpltCallback (Thumb, 120 bytes, Stack size 0 bytes, usart.o(i.HAL_UART_RxCpltCallback))
  [Called By]

  - >> UART_Receive_IT

  HAL_UART_TxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_TxCpltCallback))
  [Called By]

  - >> UART_EndTransmit_IT

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  RTC_IRQHandler (Thumb, 78 bytes, Stack size 8 bytes, rtc.o(i.RTC_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = RTC_IRQHandler ⇒ rtc_get_time ⇒ rtc_get_week
  [Calls]
  - >> rtc_get_time
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32f1xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = SysTick_Handler
  [Calls]
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  SystemInit (Thumb, 70 bytes, Stack size 0 bytes, system_stm32f1xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(.text)

  TIM6_IRQHandler (Thumb, 34 bytes, Stack size 0 bytes, main.o(i.TIM6_IRQHandler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM_Base_SetConfig (Thumb, 134 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_Init
  - >> HAL_TIM_Base_Init

  TIM_CCxChannelCmd (Thumb, 34 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_CCxChannelCmd))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_CCxChannelCmd
  [Called By]
  - >> HAL_TIM_PWM_Start

  TIM_OC2_SetConfig (Thumb, 114 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC2_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC2_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  USART1_IRQHandler (Thumb, 56 bytes, Stack size 8 bytes, usart.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = USART1_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ HAL_DMA_Abort_IT
  [Calls]
  - >> HAL_UART_Receive_IT
  - >> HAL_UART_IRQHandler
  - >> HAL_UART_GetState
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  USART2_IRQHandler (Thumb, 44 bytes, Stack size 8 bytes, usart2.o(i.USART2_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = USART2_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ HAL_DMA_Abort_IT
  [Calls]
  - >> HAL_UART_IRQHandler
  - >> ringbuffer_in_check
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  _sys_exit (Thumb, 4 bytes, Stack size 0 bytes, usart.o(i._sys_exit))
  [Called By]

  - >> __rt_exit_exit

  api_ack (Thumb, 20 bytes, Stack size 8 bytes, hmi_cmd.o(i.api_ack))
  [Stack]

  - Max Depth = 408 + Unknown Stack Size
  - Call Chain = api_ack ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_wait_parse
  - >> hmi_cmd_send
  - >> _wait_parse_idle
  [Called By]
  - >> hmi_test_init

  api_caddt (Thumb, 46 bytes, Stack size 152 bytes, hmi_cmd.o(i.api_caddt))
  [Stack]

  - Max Depth = 552 + Unknown Stack Size
  - Call Chain = api_caddt ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_wait_parse
  - >> hmi_cmd_send
  - >> _wait_parse_idle
  - >> __2snprintf
  [Called By]
  - >> real_time_curve

  api_cclear (Thumb, 32 bytes, Stack size 144 bytes, hmi_cmd.o(i.api_cclear))
  [Stack]

  - Max Depth = 264 + Unknown Stack Size
  - Call Chain = api_cclear ⇒ __2snprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> hmi_cmd_send
  - >> __2snprintf
  [Called By]
  - >> hmi_curve_example_hex_cmd

  api_get (Thumb, 38 bytes, Stack size 136 bytes, hmi_cmd.o(i.api_get))
  [Stack]

  - Max Depth = 536 + Unknown Stack Size
  - Call Chain = api_get ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_wait_parse
  - >> hmi_cmd_send
  - >> _wait_parse_idle
  - >> __2snprintf
  [Called By]
  - >> hmi_test_init
  - >> hmi_spinner_example_hex_cmd
  - >> hmi_slider_example_hex_cmd
  - >> hmi_select_text_example_hex_cmd
  - >> hmi_progerss_bar_example_timer_update_50ms
  - >> hmi_btn_example_hex_cmd

  api_get_code (Thumb, 20 bytes, Stack size 8 bytes, hmi_cmd.o(i.api_get_code))
  [Stack]

  - Max Depth = 408 + Unknown Stack Size
  - Call Chain = api_get_code ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_wait_parse
  - >> hmi_cmd_send
  - >> _wait_parse_idle
  [Called By]
  - >> hmi_test_init

  api_reset (Thumb, 20 bytes, Stack size 8 bytes, hmi_cmd.o(i.api_reset))
  [Stack]

  - Max Depth = 408 + Unknown Stack Size
  - Call Chain = api_reset ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_wait_parse
  - >> hmi_cmd_send
  - >> _wait_parse_idle
  [Called By]
  - >> main

  api_rtcs (Thumb, 46 bytes, Stack size 176 bytes, hmi_cmd.o(i.api_rtcs))
  [Stack]

  - Max Depth = 296 + Unknown Stack Size
  - Call Chain = api_rtcs ⇒ __2snprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> hmi_cmd_send
  - >> __2snprintf
  [Called By]
  - >> hmi_select_text_example_hex_cmd

  api_version (Thumb, 20 bytes, Stack size 8 bytes, hmi_cmd.o(i.api_version))
  [Stack]

  - Max Depth = 408 + Unknown Stack Size
  - Call Chain = api_version ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_wait_parse
  - >> hmi_cmd_send
  - >> _wait_parse_idle
  [Called By]
  - >> hmi_test_init

  fputc (Thumb, 24 bytes, Stack size 0 bytes, usart.o(i.fputc))
  [Address Reference Count : 1]

  - _printf_char_file.o(.text)

  hmi_btn_example_hex_cmd (Thumb, 92 bytes, Stack size 24 bytes, hmi_btn_example.o(i.hmi_btn_example_hex_cmd))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size + In Cycle
  - Call Chain = hmi_btn_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_send
  - >> hmi_cmd_back_res
  - >> api_get
  - >> __2sprintf
  - >> __2printf
  [Called By]
  - >> hmi_hex_cmd_parse

  hmi_btn_example_str_cmd (Thumb, 64 bytes, Stack size 16 bytes, hmi_btn_example.o(i.hmi_btn_example_str_cmd))
  [Stack]

  - Max Depth = 28
  - Call Chain = hmi_btn_example_str_cmd ⇒ strstr
  [Calls]
  - >> led0_set_duty
  - >> strstr
  [Called By]
  - >> hmi_str_cmd_parse

  hmi_btn_example_timer_update_50ms (Thumb, 150 bytes, Stack size 16 bytes, hmi_btn_example.o(i.hmi_btn_example_timer_update_50ms))
  [Stack]

  - Max Depth = 136 + Unknown Stack Size
  - Call Chain = hmi_btn_example_timer_update_50ms ⇒ __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> hmi_cmd_send
  - >> __2sprintf
  [Called By]
  - >> hmi_update_ui_50ms

  hmi_cmd_back_res (Thumb, 8 bytes, Stack size 8 bytes, hmi_cmd.o(i.hmi_cmd_back_res))
  [Stack]

  - Max Depth = 8
  - Call Chain = hmi_cmd_back_res
  [Calls]
  - >> hmi_rx_parse_get_res
  [Called By]
  - >> hmi_test_init
  - >> real_time_curve
  - >> hmi_spinner_example_hex_cmd
  - >> hmi_slider_example_hex_cmd
  - >> hmi_select_text_example_hex_cmd
  - >> hmi_progerss_bar_example_timer_update_50ms
  - >> hmi_btn_example_hex_cmd

  hmi_cmd_send (Thumb, 36 bytes, Stack size 16 bytes, hmi_cmd.o(i.hmi_cmd_send))
  [Stack]

  - Max Depth = 24
  - Call Chain = hmi_cmd_send ⇒ usart2_send_data
  [Calls]
  - >> usart2_send_data
  - >> strlen
  [Called By]
  - >> api_version
  - >> api_rtcs
  - >> api_get_code
  - >> api_get
  - >> api_cclear
  - >> api_caddt
  - >> api_ack
  - >> api_reset
  - >> hmi_spinner_example_hex_cmd
  - >> hmi_qr_example_hex_cmd
  - >> hmi_progerss_bar_example_timer_update_50ms
  - >> hmi_pointer_example_timer_update_50ms
  - >> hmi_btn_example_timer_update_50ms
  - >> hmi_btn_example_hex_cmd

  hmi_cmd_wait_parse (Thumb, 60 bytes, Stack size 16 bytes, hmi_cmd.o(i.hmi_cmd_wait_parse))
  [Stack]

  - Max Depth = 400 + Unknown Stack Size
  - Call Chain = hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_rx_parse_set_cmd_code
  - >> HAL_GetTick
  - >> hmi_rx_parse_task
  [Called By]
  - >> api_version
  - >> api_get_code
  - >> api_get
  - >> api_caddt
  - >> api_ack
  - >> api_reset
  - >> real_time_curve

  hmi_curve_example_hex_cmd (Thumb, 94 bytes, Stack size 16 bytes, hmi_curve_example.o(i.hmi_curve_example_hex_cmd))
  [Stack]

  - Max Depth = 280 + Unknown Stack Size
  - Call Chain = hmi_curve_example_hex_cmd ⇒ api_cclear ⇒ __2snprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> api_cclear
  [Called By]
  - >> hmi_hex_cmd_parse

  hmi_curve_example_timer_update_50ms (Thumb, 110 bytes, Stack size 8 bytes, hmi_curve_example.o(i.hmi_curve_example_timer_update_50ms))
  [Stack]

  - Max Depth = 592 + Unknown Stack Size
  - Call Chain = hmi_curve_example_timer_update_50ms ⇒ real_time_curve ⇒ api_caddt ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> real_time_curve
  [Called By]
  - >> hmi_update_ui_50ms

  hmi_hex_cmd_parse (Thumb, 84 bytes, Stack size 8 bytes, hmi_test.o(i.hmi_hex_cmd_parse))
  [Stack]

  - Max Depth = 352 + Unknown Stack Size
  - Call Chain = hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_spinner_example_hex_cmd
  - >> hmi_slider_example_hex_cmd
  - >> hmi_select_text_example_hex_cmd
  - >> hmi_qr_example_hex_cmd
  - >> hmi_curve_example_hex_cmd
  - >> hmi_btn_example_hex_cmd
  [Called By]
  - >> hmi_hex_parse_byte_to_byte

  hmi_hex_parse_byte_to_byte (Thumb, 202 bytes, Stack size 16 bytes, hmi_hex_parse.o(i.hmi_hex_parse_byte_to_byte))
  [Stack]

  - Max Depth = 368 + Unknown Stack Size
  - Call Chain = hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_hex_cmd_parse
  [Called By]
  - >> hmi_rx_parse_task

  hmi_hex_parse_reest (Thumb, 8 bytes, Stack size 0 bytes, hmi_hex_parse.o(i.hmi_hex_parse_reest))
  [Called By]

  - >> hmi_rx_parse_task

  hmi_pointer_example_timer_update_50ms (Thumb, 104 bytes, Stack size 64 bytes, hmi_pointer_example.o(i.hmi_pointer_example_timer_update_50ms))
  [Stack]

  - Max Depth = 184 + Unknown Stack Size
  - Call Chain = hmi_pointer_example_timer_update_50ms ⇒ __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> hmi_cmd_send
  - >> __2sprintf
  [Called By]
  - >> hmi_update_ui_50ms

  hmi_progerss_bar_example_timer_update_50ms (Thumb, 56 bytes, Stack size 16 bytes, hmi_progerss_bar_example.o(i.hmi_progerss_bar_example_timer_update_50ms))
  [Stack]

  - Max Depth = 552 + Unknown Stack Size
  - Call Chain = hmi_progerss_bar_example_timer_update_50ms ⇒ api_get ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_send
  - >> hmi_cmd_back_res
  - >> api_get
  - >> __2printf
  [Called By]
  - >> hmi_update_ui_50ms

  hmi_qr_example_hex_cmd (Thumb, 38 bytes, Stack size 64 bytes, hmi_qr_example.o(i.hmi_qr_example_hex_cmd))
  [Stack]

  - Max Depth = 184 + Unknown Stack Size
  - Call Chain = hmi_qr_example_hex_cmd ⇒ __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> hmi_cmd_send
  - >> __aeabi_memclr4
  - >> __2sprintf
  [Called By]
  - >> hmi_hex_cmd_parse

  hmi_rx_parse_get_res (Thumb, 4 bytes, Stack size 0 bytes, hmi_rx_parse.o(i.hmi_rx_parse_get_res))
  [Called By]

  - >> hmi_cmd_back_res

  hmi_rx_parse_set_cmd_code (Thumb, 6 bytes, Stack size 0 bytes, hmi_rx_parse.o(i.hmi_rx_parse_set_cmd_code))
  [Called By]

  - >> hmi_cmd_wait_parse

  hmi_rx_parse_task (Thumb, 104 bytes, Stack size 16 bytes, hmi_rx_parse.o(i.hmi_rx_parse_task))
  [Stack]

  - Max Depth = 384 + Unknown Stack Size
  - Call Chain = hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> usart2_get_rx_data
  - >> hmi_hex_parse_reest
  - >> hmi_hex_parse_byte_to_byte
  - >> _cmd_rx_parse_task
  - >> _buf_rest
  - >> HAL_GetTick
  [Called By]
  - >> hmi_cmd_wait_parse
  - >> _wait_parse_idle
  - >> main

  hmi_select_text_example_hex_cmd (Thumb, 234 bytes, Stack size 48 bytes, hmi_select_text_example.o(i.hmi_select_text_example_hex_cmd))
  [Stack]

  - Max Depth = 344 + Unknown Stack Size + In Cycle
  - Call Chain = hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_back_res
  - >> api_rtcs
  - >> api_get
  - >> rtc_set_time
  [Called By]
  - >> hmi_hex_cmd_parse

  hmi_slider_example_hex_cmd (Thumb, 82 bytes, Stack size 24 bytes, hmi_slider_example.o(i.hmi_slider_example_hex_cmd))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size + In Cycle
  - Call Chain = hmi_slider_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_back_res
  - >> api_get
  - >> __2printf
  [Called By]
  - >> hmi_hex_cmd_parse

  hmi_spinner_example_hex_cmd (Thumb, 100 bytes, Stack size 24 bytes, hmi_spinner_example.o(i.hmi_spinner_example_hex_cmd))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size + In Cycle
  - Call Chain = hmi_spinner_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_send
  - >> hmi_cmd_back_res
  - >> api_get
  - >> __2printf
  [Called By]
  - >> hmi_hex_cmd_parse

  hmi_str_cmd_parse (Thumb, 52 bytes, Stack size 8 bytes, hmi_test.o(i.hmi_str_cmd_parse))
  [Stack]

  - Max Depth = 232
  - Call Chain = hmi_str_cmd_parse ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_string
  [Calls]
  - >> hmi_btn_example_str_cmd
  - >> strstr
  - >> __0sscanf
  [Called By]
  - >> _cmd_return_parse

  hmi_test_init (Thumb, 92 bytes, Stack size 16 bytes, hmi_test.o(i.hmi_test_init))
  [Stack]

  - Max Depth = 552 + Unknown Stack Size
  - Call Chain = hmi_test_init ⇒ api_get ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_cmd_back_res
  - >> api_version
  - >> api_get_code
  - >> api_get
  - >> api_ack
  - >> __2printf
  [Called By]
  - >> main

  hmi_update_ui_100ms (Thumb, 2 bytes, Stack size 0 bytes, hmi_test.o(i.hmi_update_ui_100ms))
  [Called By]

  - >> main

  hmi_update_ui_50ms (Thumb, 44 bytes, Stack size 8 bytes, hmi_test.o(i.hmi_update_ui_50ms))
  [Stack]

  - Max Depth = 600 + Unknown Stack Size
  - Call Chain = hmi_update_ui_50ms ⇒ hmi_curve_example_timer_update_50ms ⇒ real_time_curve ⇒ api_caddt ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_progerss_bar_example_timer_update_50ms
  - >> hmi_pointer_example_timer_update_50ms
  - >> hmi_curve_example_timer_update_50ms
  - >> hmi_btn_example_timer_update_50ms
  [Called By]
  - >> main

  led0_pwm_init (Thumb, 198 bytes, Stack size 64 bytes, led0_pwm.o(i.led0_pwm_init))
  [Stack]

  - Max Depth = 140
  - Call Chain = led0_pwm_init ⇒ HAL_TIM_PWM_Init ⇒ HAL_TIM_PWM_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  - >> HAL_TIM_PWM_Start
  - >> HAL_TIM_PWM_Init
  - >> HAL_TIM_PWM_ConfigChannel
  [Called By]
  - >> main

  led0_set_duty (Thumb, 6 bytes, Stack size 0 bytes, led0_pwm.o(i.led0_set_duty))
  [Called By]

  - >> hmi_btn_example_str_cmd

  led_init (Thumb, 132 bytes, Stack size 24 bytes, led.o(i.led_init))
  [Stack]

  - Max Depth = 60
  - Call Chain = led_init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  main (Thumb, 166 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 600 + Unknown Stack Size
  - Call Chain = main ⇒ hmi_update_ui_50ms ⇒ hmi_curve_example_timer_update_50ms ⇒ real_time_curve ⇒ api_caddt ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> usart_init
  - >> usart2_init
  - >> timer6_init
  - >> sys_stm32_clock_init
  - >> rtc_init
  - >> led_init
  - >> led0_pwm_init
  - >> hmi_update_ui_50ms
  - >> hmi_update_ui_100ms
  - >> hmi_test_init
  - >> hmi_rx_parse_task
  - >> api_reset
  - >> HAL_Init
  - >> HAL_GPIO_TogglePin
  - >> millis
  [Called By]
  - >> __rt_entry_main

  millis (Thumb, 6 bytes, Stack size 0 bytes, main.o(i.millis))
  [Called By]

  - >> main

  ringbuffer_getRemainSize (Thumb, 20 bytes, Stack size 4 bytes, ringbuffer.o(i.ringbuffer_getRemainSize))
  [Stack]

  - Max Depth = 4
  - Call Chain = ringbuffer_getRemainSize
  [Calls]
  - >> ringbuffer_getUsedSize
  [Called By]
  - >> ringbuffer_in_check

  ringbuffer_getUsedSize (Thumb, 34 bytes, Stack size 0 bytes, ringbuffer.o(i.ringbuffer_getUsedSize))
  [Called By]

  - >> ringbuffer_out
  - >> ringbuffer_getRemainSize

  ringbuffer_in (Thumb, 40 bytes, Stack size 16 bytes, ringbuffer.o(i.ringbuffer_in))
  [Stack]

  - Max Depth = 16
  - Call Chain = ringbuffer_in
  [Called By]
  - >> ringbuffer_in_check

  ringbuffer_in_check (Thumb, 38 bytes, Stack size 20 bytes, ringbuffer.o(i.ringbuffer_in_check))
  [Stack]

  - Max Depth = 36
  - Call Chain = ringbuffer_in_check ⇒ ringbuffer_in
  [Calls]
  - >> ringbuffer_in
  - >> ringbuffer_getRemainSize
  [Called By]
  - >> USART2_IRQHandler

  ringbuffer_init (Thumb, 12 bytes, Stack size 0 bytes, ringbuffer.o(i.ringbuffer_init))
  [Called By]

  - >> usart2_init

  ringbuffer_out (Thumb, 60 bytes, Stack size 20 bytes, ringbuffer.o(i.ringbuffer_out))
  [Stack]

  - Max Depth = 20
  - Call Chain = ringbuffer_out
  [Calls]
  - >> ringbuffer_getUsedSize
  [Called By]
  - >> usart2_get_rx_data

  rtc_get_time (Thumb, 254 bytes, Stack size 32 bytes, rtc.o(i.rtc_get_time))
  [Stack]

  - Max Depth = 48
  - Call Chain = rtc_get_time ⇒ rtc_get_week
  [Calls]
  - >> rtc_get_week
  - >> rtc_is_leap_year
  [Called By]
  - >> rtc_init
  - >> RTC_IRQHandler

  rtc_get_week (Thumb, 80 bytes, Stack size 16 bytes, rtc.o(i.rtc_get_week))
  [Stack]

  - Max Depth = 16
  - Call Chain = rtc_get_week
  [Called By]
  - >> rtc_get_time

  rtc_init (Thumb, 174 bytes, Stack size 16 bytes, rtc.o(i.rtc_init))
  [Stack]

  - Max Depth = 144
  - Call Chain = rtc_init ⇒ HAL_RTC_Init ⇒ HAL_RTC_MspInit ⇒ HAL_RCC_OscConfig ⇒ RCC_Delay
  [Calls]
  - >> HAL_PWR_EnableBkUpAccess
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> rtc_set_time
  - >> rtc_read_bkr
  - >> rtc_get_time
  - >> HAL_RTC_Init
  [Called By]
  - >> main

  rtc_read_bkr (Thumb, 20 bytes, Stack size 16 bytes, rtc.o(i.rtc_read_bkr))
  [Stack]

  - Max Depth = 24
  - Call Chain = rtc_read_bkr ⇒ HAL_RTCEx_BKUPRead
  [Calls]
  - >> HAL_RTCEx_BKUPRead
  [Called By]
  - >> rtc_init

  rtc_set_time (Thumb, 154 bytes, Stack size 40 bytes, rtc.o(i.rtc_set_time))
  [Stack]

  - Max Depth = 92
  - Call Chain = rtc_set_time ⇒ rtc_date2sec
  [Calls]
  - >> HAL_PWR_EnableBkUpAccess
  - >> rtc_date2sec
  [Called By]
  - >> rtc_init
  - >> hmi_select_text_example_hex_cmd

  rtc_write_bkr (Thumb, 22 bytes, Stack size 16 bytes, rtc.o(i.rtc_write_bkr))
  [Stack]

  - Max Depth = 24
  - Call Chain = rtc_write_bkr ⇒ HAL_RTCEx_BKUPWrite
  [Calls]
  - >> HAL_PWR_EnableBkUpAccess
  - >> HAL_RTCEx_BKUPWrite
  [Called By]
  - >> HAL_RTC_MspInit

  sys_stm32_clock_init (Thumb, 86 bytes, Stack size 72 bytes, sys.o(i.sys_stm32_clock_init))
  [Stack]

  - Max Depth = 152
  - Call Chain = sys_stm32_clock_init ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  [Called By]
  - >> main

  timer6_init (Thumb, 80 bytes, Stack size 16 bytes, time6.o(i.timer6_init))
  [Stack]

  - Max Depth = 64
  - Call Chain = timer6_init ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_TIM_Base_Start_IT
  - >> HAL_TIM_Base_Init
  [Called By]
  - >> main

  usart2_get_rx_data (Thumb, 18 bytes, Stack size 16 bytes, usart2.o(i.usart2_get_rx_data))
  [Stack]

  - Max Depth = 36
  - Call Chain = usart2_get_rx_data ⇒ ringbuffer_out
  [Calls]
  - >> ringbuffer_out
  [Called By]
  - >> hmi_rx_parse_task

  usart2_init (Thumb, 202 bytes, Stack size 32 bytes, usart2.o(i.usart2_init))
  [Stack]

  - Max Depth = 120
  - Call Chain = usart2_init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_UART_Init
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  - >> ringbuffer_init
  [Called By]
  - >> main

  usart2_send_data (Thumb, 42 bytes, Stack size 8 bytes, usart2.o(i.usart2_send_data))
  [Stack]

  - Max Depth = 8
  - Call Chain = usart2_send_data
  [Called By]
  - >> hmi_cmd_send
  - >> real_time_curve

  usart_init (Thumb, 44 bytes, Stack size 8 bytes, usart.o(i.usart_init))
  [Stack]

  - Max Depth = 96
  - Call Chain = usart_init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_UART_Receive_IT
  - >> HAL_UART_Init
  [Called By]
  - >> main

  _get_lc_ctype (Thumb, 44 bytes, Stack size 8 bytes, lc_ctype_c.o(locale$$code))
  [Stack]

  - Max Depth = 8
  - Call Chain = _get_lc_ctype
  [Calls]
  - >> strcmp
  [Called By]
  - >> __rt_lib_init_lc_ctype_2
  [Address Reference Count : 1]
  - rt_ctype_table.o(.text)

  ### Local Symbols

  _wait_parse_idle (Thumb, 16 bytes, Stack size 8 bytes, hmi_cmd.o(i._wait_parse_idle))
  [Stack]

  - Max Depth = 392 + Unknown Stack Size
  - Call Chain = _wait_parse_idle ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> hmi_rx_parse_task
  [Called By]
  - >> api_version
  - >> api_get_code
  - >> api_get
  - >> api_caddt
  - >> api_ack
  - >> api_reset

  _buf_rest (Thumb, 10 bytes, Stack size 0 bytes, hmi_rx_parse.o(i._buf_rest))
  [Called By]

  - >> _cmd_rx_parse_task
  - >> hmi_rx_parse_task

  _buf_save_res_buf (Thumb, 50 bytes, Stack size 16 bytes, hmi_rx_parse.o(i._buf_save_res_buf))
  [Stack]

  - Max Depth = 24
  - Call Chain = _buf_save_res_buf ⇒ strlen
  [Calls]
  - >> __aeabi_memmove
  - >> strlen
  - >> strchr
  [Called By]
  - >> _cmd_return_parse

  _cmd_return_parse (Thumb, 248 bytes, Stack size 24 bytes, hmi_rx_parse.o(i._cmd_return_parse))
  [Stack]

  - Max Depth = 256
  - Call Chain = _cmd_return_parse ⇒ hmi_str_cmd_parse ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_string
  [Calls]
  - >> _buf_save_res_buf
  - >> hmi_str_cmd_parse
  - >> strstr
  - >> __0sscanf
  [Called By]
  - >> _cmd_rx_parse_task

  _cmd_rx_parse_task (Thumb, 136 bytes, Stack size 16 bytes, hmi_rx_parse.o(i._cmd_rx_parse_task))
  [Stack]

  - Max Depth = 272
  - Call Chain = _cmd_rx_parse_task ⇒ _cmd_return_parse ⇒ hmi_str_cmd_parse ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_string
  [Calls]
  - >> _cmd_return_parse
  - >> _buf_rest
  [Called By]
  - >> hmi_rx_parse_task

  __NVIC_GetPriorityGrouping (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.__NVIC_GetPriorityGrouping))
  [Called By]

  - >> HAL_NVIC_SetPriority

  __NVIC_SetPriority (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.__NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = __NVIC_SetPriority
  [Called By]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  RCC_Delay (Thumb, 36 bytes, Stack size 8 bytes, stm32f1xx_hal_rcc.o(i.RCC_Delay))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_Delay
  [Called By]
  - >> HAL_RCC_OscConfig

  UART_DMAAbortOnError (Thumb, 20 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_DMAAbortOnError
  [Calls]
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler)

  UART_EndRxTransfer (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.UART_EndRxTransfer))
  [Called By]

  - >> HAL_UART_IRQHandler

  UART_EndTransmit_IT (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.UART_EndTransmit_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_EndTransmit_IT
  [Calls]
  - >> HAL_UART_TxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_Receive_IT (Thumb, 166 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.UART_Receive_IT))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_Receive_IT
  [Calls]
  - >> HAL_UART_RxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_SetConfig (Thumb, 412 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> HAL_UART_Init

  UART_Transmit_IT (Thumb, 104 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.UART_Transmit_IT))
  [Called By]

  - >> HAL_UART_IRQHandler

  TIM_OC1_SetConfig (Thumb, 104 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC1_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC1_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC3_SetConfig (Thumb, 112 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC3_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC3_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC4_SetConfig (Thumb, 74 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC4_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC4_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  RTC_EnterInitMode (Thumb, 58 bytes, Stack size 16 bytes, stm32f1xx_hal_rtc.o(i.RTC_EnterInitMode))
  [Stack]

  - Max Depth = 16
  - Call Chain = RTC_EnterInitMode
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RTC_Init

  RTC_ExitInitMode (Thumb, 58 bytes, Stack size 16 bytes, stm32f1xx_hal_rtc.o(i.RTC_ExitInitMode))
  [Stack]

  - Max Depth = 16
  - Call Chain = RTC_ExitInitMode
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RTC_Init

  rtc_date2sec (Thumb, 166 bytes, Stack size 52 bytes, rtc.o(i.rtc_date2sec))
  [Stack]

  - Max Depth = 52
  - Call Chain = rtc_date2sec
  [Called By]
  - >> rtc_set_time

  rtc_is_leap_year (Thumb, 50 bytes, Stack size 0 bytes, rtc.o(i.rtc_is_leap_year))
  [Called By]

  - >> rtc_get_time

  real_time_curve (Thumb, 98 bytes, Stack size 32 bytes, hmi_curve_example.o(i.real_time_curve))
  [Stack]

  - Max Depth = 584 + Unknown Stack Size
  - Call Chain = real_time_curve ⇒ api_caddt ⇒ hmi_cmd_wait_parse ⇒ hmi_rx_parse_task ⇒ hmi_hex_parse_byte_to_byte ⇒ hmi_hex_cmd_parse ⇒ hmi_select_text_example_hex_cmd ⇒ api_get (Cycle)
  [Calls]
  - >> usart2_send_data
  - >> hmi_cmd_wait_parse
  - >> hmi_cmd_back_res
  - >> api_caddt
  - >> strstr
  [Called By]
  - >> hmi_curve_example_timer_update_50ms

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  _scanf_char_input (Thumb, 12 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Address Reference Count : 1]

  - scanf_char.o(.text)

  ### Undefined Global Symbols